From 5b70aa8b4809baa25e40fa4edff5c7ad60cf91aa Mon Sep 17 00:00:00 2001
From: "Matthias P. Braendli" <matthias.braendli@mpb.li>
Date: Fri, 20 Mar 2015 08:25:54 +0100
Subject: Fix hackrf configuration output

---
 scenarios.tex | 6 ++----
 1 file changed, 2 insertions(+), 4 deletions(-)

(limited to 'scenarios.tex')

diff --git a/scenarios.tex b/scenarios.tex
index a841035..d452f99 100644
--- a/scenarios.tex
+++ b/scenarios.tex
@@ -189,13 +189,12 @@ output=file
 
 [fileoutput]
 format=s8
-filename=/dev/stdout
+filename=/tmp/ofdm.fifo
 
 \end{lstlisting}
 
 The output fifo has to be created beforehand, and the \texttt{hackrf\_transfer}
-utility is then used to transmit the signal to the device. The options needed
-for the transmission utility are not complete yet. The rough idea would be:
+utility is then used to transmit the signal to the device.
 
 Depending on the capabilities of the host computer, using higher sampling rates
 ($6144$k, and even $8192$k) may be possible. This oversampling is desirable as
@@ -209,7 +208,6 @@ equivalent to that obtained from first generation commercial modulators. This
 can be increased to a relatively respectable $\approx 40$dB by enabling the FIR filter
 in ODR-DabMod, and an appropriate coefficient file provided.
 
-
 Example of using ODR-DabMod with the \texttt{hackrf\_transfer} utility:
 
 \begin{lstlisting}
-- 
cgit v1.2.3

