From 8d60e3486dd6b0f2dc72223dc3f660d5d6ab8e00 Mon Sep 17 00:00:00 2001
From: "Matthias P. Braendli" <matthias.braendli@mpb.li>
Date: Sat, 16 Feb 2019 17:00:24 +0100
Subject: Mention TX Antenna for LimeSDR Mini

---
 scenarios.tex | 3 +++
 1 file changed, 3 insertions(+)

(limited to 'scenarios.tex')

diff --git a/scenarios.tex b/scenarios.tex
index 285eca6..3afbaa8 100644
--- a/scenarios.tex
+++ b/scenarios.tex
@@ -157,6 +157,9 @@ The available sampling rates, the TX gain range and the antenna selection are
 device-specific, and can be discovered using the \texttt{SoapySDRUtil --probe}
 command.
 
+For example, the LimeSDR mini requires the \verb+tx_antenna+ to be set to
+BAND2.
+
 \subsubsection{HackRF Through Stdout Pipe}
 For devices that are not offering a SoapySDR device driver, the last resort is
 to use standard output or a fifo to carry the IQ data from ODR-DabMod to a tool
-- 
cgit v1.2.3

