From a60909ae99e5bfb24497d39119984c7dcdeb1202 Mon Sep 17 00:00:00 2001
From: "Matthias P. Braendli" <matthias.braendli@mpb.li>
Date: Wed, 4 Oct 2017 13:12:06 +0200
Subject: Add section about resource usage

---
 scenarios.tex | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

(limited to 'scenarios.tex')

diff --git a/scenarios.tex b/scenarios.tex
index ba55533..b28e3b5 100644
--- a/scenarios.tex
+++ b/scenarios.tex
@@ -146,6 +146,7 @@ it in steps of $3$dB or smaller while measuring the output signal, until the
 correct power is reached.
 
 \subsubsection{Other Hardware}
+\label{otherhardware}
 ODR-DabMod supports other radio interfaces using SoapySDR or through standard output, or via
 a fifo -- the latter must be created prior to runtime with the \texttt{mkfifo} command.
 Due to limitations in the UHD driver library, \texttt{/dev/stdout} will only
@@ -165,7 +166,7 @@ chosen inside the valid range for the device being used. This range can be shown
 by calling \texttt{SoapySDRUtil --probe}.
 
 ODR-DabMod has been tested working with HackRF on i386 and
-x86 architectures.\footnote{HackRF has not been tested to any degree of success
+x86\_64 architectures.\footnote{HackRF has not been tested to any degree of success
 with ARM-based computers at this time as they are not (yet) capable of resampling
 to the required higher rates as the process is highly CPU intensive.}
 
-- 
cgit v1.2.3

