From 2d295db25e60251168d61c23ed67d3f23f2a863c Mon Sep 17 00:00:00 2001
From: Rash <rashid.mustapha@gmail.com>
Date: Mon, 13 Apr 2015 13:21:47 +0100
Subject: Another typo.

---
 scenarios.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'scenarios.tex')

diff --git a/scenarios.tex b/scenarios.tex
index 8d53ec6..a0383b9 100644
--- a/scenarios.tex
+++ b/scenarios.tex
@@ -233,7 +233,7 @@ Rate        Dgain   Max Dgain (Empirical)
 8192 ksps    4.0     4.50
 
 The shoulder performance has been measured with shoulder performance at a little
-better than 35$dB, which is roughly equivalent to that obtained from first 
+better than $35$dB, which is roughly equivalent to that obtained from first 
 generation commercial modulator equipment. This can be increased to a relatively 
 respectable $\approx 40$dB by enabling the FIR baseband filter in ODR-DabMod, 
 and supplying it with an appropriate coefficient (tap) file. The maximum output
-- 
cgit v1.2.3

