From c89848ee86a718ab4d58cea485773baee00628da Mon Sep 17 00:00:00 2001
From: andimik <andimik@yahoo.de>
Date: Tue, 15 Aug 2017 22:27:22 +0200
Subject: typos fixed

---
 scenarios.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'scenarios.tex')

diff --git a/scenarios.tex b/scenarios.tex
index 54673f9..3b072bb 100644
--- a/scenarios.tex
+++ b/scenarios.tex
@@ -41,7 +41,7 @@ filename=myfirst.iq
 This is a very minimal file that defines only the necessary settings equivalent
 to the above command line options. The configuration file however supports more
 options that the command line, and becomes easier to manager once the set
-becomes more complex. It is best to use the example configuration availble in
+becomes more complex. It is best to use the example configuration available in
 the \texttt{doc/} folder.
 
 \subsection{Interfacing Hardware Devices}
@@ -252,7 +252,7 @@ better than $35$dB, which is roughly equivalent to that obtained from first
 generation commercial modulator equipment. This can be increased to a relatively
 respectable $\approx 40$dB by enabling the FIR baseband filter in ODR-DabMod,
 and supplying it with an appropriate coefficient (tap) file. The maximum output
-power available to mmet these performance figures is approximately $-10$dBm RMS.
+power available to meet these performance figures is approximately $-10$dBm RMS.
 
 Example of using ODR-DabMod with the \texttt{hackrf\_transfer} utility:
 
-- 
cgit v1.2.3

